*************************** START ****************************

START TIME: 202405061234

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x3206fdd8
mac h: 0x7eb0a7
crc_cal: 126
crc_read: 126
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 852160 bytes (486108 compressed) at 0x00010000 in 8.5 seconds (effective 802.8 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 10 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202405061243

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x3206fdd8
mac h: 0x7eb0a7
crc_cal: 126
crc_read: 126
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 852160 bytes (486108 compressed) at 0x00010000 in 8.5 seconds (effective 806.0 kbit/s)...

Hash of data verified.
Wrote 2031616 bytes (756165 compressed) at 0x00210000 in 17.0 seconds (effective 955.4 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 30 s

Download result: PASS

*************************** END ****************************



