*************************** START ****************************

START TIME: 202405061258

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xa77bed1c
mac h: 0xfccdb
crc_cal: 15
crc_read: 15
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 852160 bytes (486108 compressed) at 0x00010000 in 8.1 seconds (effective 841.8 kbit/s)...

Hash of data verified.
Wrote 2031616 bytes (756165 compressed) at 0x00210000 in 15.9 seconds (effective 1021.4 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 29 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202405061302

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xa77bed1c
mac h: 0xfccdb
crc_cal: 15
crc_read: 15
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 852160 bytes (486108 compressed) at 0x00010000 in 8.0 seconds (effective 850.8 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 10 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202405061303

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xa77bed1c
mac h: 0xfccdb
crc_cal: 15
crc_read: 15
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 852160 bytes (486108 compressed) at 0x00010000 in 8.0 seconds (effective 850.1 kbit/s)...

Hash of data verified.
Wrote 2031616 bytes (756165 compressed) at 0x00210000 in 15.8 seconds (effective 1026.4 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 39 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202405061320

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xa77bed1c
mac h: 0xfccdb
crc_cal: 15
crc_read: 15
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 852160 bytes (486108 compressed) at 0x00010000 in 8.0 seconds (effective 852.2 kbit/s)...

Hash of data verified.
Wrote 2031616 bytes (756165 compressed) at 0x00210000 in 15.8 seconds (effective 1030.4 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 28 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202405061323

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xa77bed1c
mac h: 0xfccdb
crc_cal: 15
crc_read: 15
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 852160 bytes (486108 compressed) at 0x00010000 in 7.8 seconds (effective 878.5 kbit/s)...

Hash of data verified.
Wrote 2031616 bytes (756165 compressed) at 0x00210000 in 15.5 seconds (effective 1046.0 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 46 s

Download result: PASS

*************************** END ****************************



